Corrigendum-3 to RFP No. T-11014/23/2017-Tech/Vol-1

| S. No. | *Clause No.* | RFP Pg. No. | *Clause as per RFP* | *Modified* Clause |
| --- | --- | --- | --- | --- |
| 1 | 1.2.2 | 13 | | **Area** | **Description** | | --- | --- | | Method of Selection | L 1 based upon commercial bid | | | **Area** | **Description** | | --- | --- | | Method of Selection | *L1 based upon Overall Net Present Value (NPV).*  *(However total cost of the project is on actuals mentioned in Annexure 4.2.2 & 4.2.3).* |   (Changes made only in row 1 of clause 1.2.2) |
| 2 | 1.3.2 (iv) | 15 | - | Un-priced BoQ with Model and Make ( format as mentioned in BoQ\_xxxx.xls but without any cost mentioned) |
| 3 | 2.26 (2) | 34 | Technical Bids will be opened in the presence of representatives of the Bidders (not more than two representatives per bidder) who choose to be present as per the date and time indicated by the UIDAI. Evaluation of Technical bid is subject to meeting all pre qualification criteria. A detailed evaluation will be subsequently carried out by the UIDAI. In this phase, the Technical Bids will be reviewed for compliance of the Bid requirements with reference to the responses to the technical requirements given in Section IV and schedule of requirements of this Bid Document (Section V).Technical Bids which meet the above mentioned criteria will be eligible for consideration in the subsequent rounds. If required, the UIDAI may seek specific clarifications from any or all Bidder(s) at this stage. The UIDAI shall determine the Bidders that qualify for the next phase after reviewing the clarifications provided by the Bidder(s). | Technical Bids will be opened in the presence of representatives of the Bidders (not more than two representatives per bidder) who choose to be present as per the date and time indicated by the UIDAI. Evaluation of Technical bid is subject to meeting all pre qualification criteria. A detailed evaluation will be subsequently carried out by the UIDAI. In this phase, the Technical Bids will be reviewed for compliance of the Bid requirements with reference to all the documents listed in clause 1.3.2. Technical Bids which meet the above mentioned criteria will be eligible for consideration in the subsequent rounds. If required, the UIDAI may seek specific clarifications from any or all Bidder(s) at this stage. The UIDAI shall determine the Bidders that qualify for the next phase after reviewing the clarifications provided by the Bidder(s). |
| 4 | 5.4.1 (9) | 82 | All the personnel employed by the successful bidder/Vendor for this contract shall adhere to the security policy of UIDAI/Aadhaar Act, 2016 and should follow the policy of UIDAI in terms of software, configuration and services. The security policy of UIDAI shall be shared with the successful bidder/Vendor while on-boarding. | All the personnel employed by the successful bidder/Vendor for this contract shall adhere to the IS policy of UIDAI/Aadhaar Act, 2016 and should follow the policy of UIDAI in terms of software, configuration and services. The IS policy of UIDAI shall be shared with the successful bidder/Vendor while on-boarding. |
| 5 | 6.5.4 (7) | 120 | SSL Inspection Throughput for RSA 2k – at least 5 Gbps | SSL Inspection Throughput – at least 5 Gbps |
| 6 | 3.10.1 (2) | 47 | This warranty shall remain valid, for 3 Years (36 months) in respect of equipment, or any portion thereof as the case may be, which have been delivered (and commissioned) to the final destination indicated and accepted as part of the scope of this bid. The warranty period shall commence from the date of acceptance of system i.e. UAT of all the devices by UIDAI after the successful installation and commissioning of the same or 30 days after submission of ATRR by the bidder, whichever is earlier. In case if the warranty commences without UAT, then also, UAT is to be carried out during the currency of warranty at the earliest date. In case if UAT commences within 30 days of ATRR but is not successful due to default by vendor, in that case, warranty shall be shifted for the duration during which default persisted. Please refer clause 5.4.3 (4).  **Note:**  This clause supersedes all other clauses of RFP in case of any contradiction, provided the compliance of SLA provisions (as mentioned in RFP) during the testing period shall remain unaffected by this modification.  For e.g.  If ATRR is submitted by the vendor on 1st January 2018, then UIDAI will commence the UAT on or after 1st January, 2018.  i) Scenario 1-UAT gets completed on 20th January, 2018 – Then the warranty for the equipment shall start from 21st January, 2018.  ii) Scenario 2- UAT gets completed on 20th February 2018 – then the warranty for equipment shall start from 31st January 2018. However, the terms of SLA as mentioned in Clause 5.4.3 (4) of RFP shall be applicable till the completion of UAT i.e., till 20th February 2018. | This warranty shall remain valid, for 3 Years (36 months) in respect of equipment, or any portion thereof as the case may be, which have been delivered (and commissioned) to the final destination indicated and accepted as part of the scope of this bid. The warranty period shall commence from the date of acceptance of system i.e. UAT of all the devices by UIDAI after the successful installation and commissioning of the same or 30 days after submission of ATRR by the bidder, whichever is earlier. In case if the warranty commences without UAT, then also, UAT is to be carried out during the currency of warranty at the earliest date. In case if UAT commences within 30 days of ATRR but is not successful due to default by vendor, in that case, warranty shall be shifted for the duration during which default persisted. Please refer clause 5.4.3 (4).  For e.g.  If ATRR is submitted by the vendor on 1st January 2018, then UIDAI will commence the UAT on or after 1st January, 2018.  i) Scenario 1-UAT gets completed on 20th January, 2018 – Then the warranty for the equipment shall start from 21st January, 2018.  ii) Scenario 2- UAT gets completed on 20th February 2018 – then the warranty for equipment shall start from 31st January 2018. However, the terms of SLA as mentioned in Clause 5.4.3 (4) of RFP shall be applicable till the completion of UAT i.e., till 20th February 2018. |
| 7 | 6.5.3 (51) | 117 | Concurrent connections – 15 Million | Concurrent connections – 12 Million |
| 8 | 6.5.5 (14) | 126 | Support at least 4K VLAN (including reserved, if any) and 96k MAC Addresses | Support at least 4K VLAN (including reserved, if any) and 92k MAC Addresses |
| 9 | 6.5.5 (31) | 127 | IGMP snooping for IPv4 and IPv6, MLD v1 & v2 snooping | IGMP snooping for IPv4 and IPv6 |